SPECIFICATIONS AG L/W40 JETTING UNIT

PERFORMACE 3600psi(250bar) @13gals (60ltrs)

PUMP Speck triplex P45

ENGINE Lombardini2204 4cylinder water cooled diesel

 With auto shut down 49HP

DRIVE Via heavy duty toothed belt

JETTING REEL 125mtr capacity hyd powered c/w 90 mtrs jetting hose and hose feed guide

INLET REEL 50mtr capacity hand wound c/w 25mtrs ¾” hose

TANK 400ltr capacity polythene

FUEL CAPACITY 29 ltrs

CONTROLS All mounted close to hose reel

DIMENSIONS 1300mm x 1350mm x 1500mmH

WEIGHT 540kg